**Bios update on shell**

Please check your bios version before updating. If your bios version date is 08/11/2021, there is no need to update.

Bios download link:


<https://www.mediafire.com/file/iqu574lta54aqdn/HM50HM80HM90_bios_.rar/file>




NOTE：

During the update, please don't cut off the power abnormally, and don't interrupt the update process.

1.Format the USB flash disk, format : FAT32 , name: WINPE .



2.Unzip the downloaded ‘HM50HM80HM90 bios’ file to the USB flash drive.




3. Insert the USB flash drive into the PC, After booting, Press F7 repeatedly, select “UEFI: XXXXXX”, ENTER.




4. Update in four steps


(1) fs\*: :Enter the command to find the USB flash disk: enter " fs0: " Enter, then enter "dir" to enter, Check if these files are in your USB flash drive, if not, fs1: , fs2: , fs3: ......Try again

Due to the order of the file system, the location of my USB flash drive is at fs1: 


(2) ls : Specify the drive, directory, or file to be listed.



(3)type EfiFlash.nsh : List text content



(4) AfuEfix64.efi ARM4.BIN /p /b /n /k /x /reboot : Use ARM4.BIN to start the update.



5. After the update is complete, HM80 will automatically restart, please be patient.